{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Tabelle1","Tabelle2","Tabelle3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tabelle1","index":0,"n_rows":108,"n_cols":11,"rows_kept":108,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Mode","FEC","Baud","WPM","Duty Cycle","BW (Hz)","Modulation","S/N","ITU","RSID-1","RSID-2"]
["8PSK125","-",125,620,0.8,125,"1-8PSK FM/SSB",null,"250HG1B",56,1066]
["8PSK125F","+",125,620,0.8,125,"1-8PSK FM/SSB",null,"250HG1B",56,1037]
["8PSK250","-",250,620,0.8,250,"1-8PSK FM/SSB",null,"250HG1B",56,1071]
["8PSK250F","+",250,620,0.8,250,"1-8PSK FM/SSB",null,"250HG1B",56,1038]
["8PSK500","-",500,1650,0.8,500,"1-8PSK FM",null,"500HG1B",56,1076]
["8PSK500F","+",500,1650,0.8,500,"1-8PSK FM",null,"500HG1B",56,1043]
["8PSK1000","-",1000,3300,0.8,1000,"1-8PSK FM",null,"1000HG1B",56,1047]
["8PSK1000F","+",1000,3300,0.8,1000,"1-8PSK FM",null,"1000HG1B",56,1078]
["8PSK1200F","+",1200,4200,0.8,1200,"1-8PSK FM",null,"1200HG1B",56,1058]
["CONTESTIA-4-25","+","62,5",40,1,250,"4-FSK","-10dB","250HF1B",55,"-"]
["CONTESTIA-4-50","+",125,78,1,500,"4-FSK","-8dB","500HF1B",54,"-"]
["CONTESTIA-8-10","+",125,117,1,1000,"8-FSK","-5dB","1K00F1B",117,"-"]
["CONTESTIA-8-250","+","31,25",30,1,250,"8-FSK","-13dB","250HF1B",49,"-"]
["CONTESTIA-8-50","+","62,5",60,1,500,"8-FSK","-10dB","500HF1B",52,"-"]
["CONTESTIA-16-1","+","62,5",78,1,1000,"16-FSK","-9dB","1K00F1B",53,"-"]
["CONTESTIA-16-5","+","31,25",30,1,500,"16-FSK","-12dB","500HF1B",50,"-"]
["CONTESTIA-32-1","+","31,25",48,1,1000,"32-FSK","-12dB","1K00F1B",51,"-"]
["CW20","-",10,20,0.44,50,"MCW",null,"50H0A1A","nein","-"]
["CW40","-",20,40,0.44,100,"MCW",null,"100HA1A","nein","-"]
["CW100","-",50,100,0.44,200,"MCW",null,"200HA1B",6,"-"]
["DominoEX4","optional","3,9",29,1,173,"IFK+",null,"173HF1B",84,"-"]
["DominoEX5","optional","5,4",44,1,244,"IFK+",null,"244HF1B",85,"-"]
["DominoEX8","optional","7,8",58,1,346,"IFK+",null,"346HF1B",86,"-"]
["DominoEX11","optional","10,8",80,1,262,"IFK+",null,"262HF1B",87,"-"]
["DominoEX16","optional","15,6",115,1,355,"IFK+",null,"355HF1B",88,"-"]
["DominoEX22","optional","21,5",160,1,524,"IFK+",null,"524HF1B",90,"-"]
["DominoEX44","optional",43,312,1,1600,"IFK+",null,"1600HF1B",263,45]
["DominoEX88","optional",86,614,1,1600,"IFK+",null,"1600HF1B",263,46]
["MFSK4","+","3,9",18,1,154,"32-FSK",null,"154HF1B",null,"-"]
["MFSK8","+","7,8",36,1,316,"32-FSK",null,"316HF1B",60,"-"]
["MFSK11","+","10,8",40,1,218,"16-FSK",null,"218HF1B",148,"-"]
["MFSK16","+","15,6",58,1,316,"16-FSK",null,"316HF1B",57,"-"]
["MFSK22","+","21,5",80,1,435,"16-FSK",null,"435HF1B",152,"-"]
["MFSK31","+","31,3",55,1,330,"8-FSK",null,"330HF1B",null,"-"]
["MFSK32","+","31,3",120,1,630,"16-FSK",null,"630HF1B",147,"-"]
["MFSK64","+",63,240,1,1260,"16-FSK",null,"1260HF1B",263,30]
["MFSK128","+",125,480,1,1920,null,null,"1920HF1B",263,31]
["MT63-500","+",5,50,0.8,500,"64 x 2-PSK",null,"500HJ2DE",9,"-"]
["MT63-1000","+",10,100,0.8,1000,"64 x 2-PSK",null,"1K00J2DEN",12,"-"]
["MT63-2000","+",20,200,0.8,2000,"64 x 2-PSK",null,"2K00J2DEN",15,"-"]
["OLIVIA-4-250","+",63,20,1,250,"4-FSK","-12dB","250HF1B",75,"-"]
["OLIVIA-4-500","+",125,40,1,500,"4-FSK","-10dB","500HF1B",74,"-"]
["OLIVIA-8-1000","+",125,58,1,1000,"8-FSK","-7dB","1K00F1B",116,"-"]
["OLIVIA-8-250","+",31,15,1,250,"8-FSK","-14dB","250HF1B",69,"-"]
["OLIVIA-8-500","+",63,30,1,500,"8-FSK","-11dB","500HF1B",72,"-"]
["OLIVIA-16-1000","+",63,40,1,1000,"16-FSK","-10dB","1K00F1B",73,"-"]
["OLIVIA-16-500","+",31,20,1,500,"16-FSK","-13dB","500HF1B",70,"-"]
["OLIVIA-32-1000","+",31,24,1,1000,"32-FSK","-12dB","1K00F1B",71,"-"]
["PSK31","-",31.25,50,0.8,31,"1-PSK",null,"31HG1B",1,"-"]
["PSK63","-",62.5,100,0.8,63,"1-PSK",null,"63HG1B",2,"-"]
["PSK63FEC","+",62.5,55,0.8,63,"1-PSK",null,"63HG1B",22,"-"]
["PSK63RC4","-",63,220,0.8,330,"4-PSK4",null,"330HG1BC",263,1]
["PSK63RC5","-",63,275,0.8,416,"5-PSKR",null,"416HG1BC",263,2]
["PSK63RC10","-",63,550,0.8,850,"10-PSKR",null,"850HG1BC",263,3]
["PSK63RC20","-",63,1100,0.8,1725,"20-PSKR",null,"1725HG1B",263,4]
["PSK63RC32","-",63,1760,0.8,2775,"32-PSKR",null,"2775HG1B",263,5]
["PSK125","-",125,200,0.8,125,"1-PSK",null,"250HG1B",4,"-"]
["PSK125R","-",125,110,0.8,125,"1-PSKR",null,"250HG1B",183,"-"]
["PSK125RC10","-",125,1100,0.8,1700,"10-PSKR",null,"1700HG1B",12,"-"]
["PSK125RC16","-",125,1760,0.8,2750,"16-PSKR",null,"2750HG1B",13,"-"]
["PSK125RC4","-",125,352,0.8,650,"3-PSKR",null,"650HG1B",10,"-"]
["PSK125RC5","-",125,440,0.8,825,"4-PSKR",null,"700HG1BC",11,"-"]
["PSK250","-",250,400,0.8,250,"1-PSK",null,"500HG1B",126,"-"]
["PSK250C6","-",250,2400,0.8,2000,"6-PSK",null,"2000HG1B",263,63]
["PSK250R","-",250,220,0.8,250,"1-PSKR",null,"500HG1B",186,"-"]
["PSK250RC2","-",250,440,0.8,600,"2-PSKR",null,"600HG1BC",263,20]
["PSK250RC3","-",250,660,0.8,950,"3-PSKR",null,"950HG1BC",263,21]
["PSK250RC5","-",250,1100,0.8,1650,"5-PSKR",null,"1760HG1B",263,22]
["PSK250RC6","-",250,1320,0.8,2000,"6-PSKR",null,"2000HG1B",263,65]
["PSK250RC7","-",250,1540,0.8,2350,"7-PSKR",null,"2350HG1B",263,23]
["PSK500","-",500,800,0.8,500,"1-PSK",null,"500HG1B",173,"-"]
["PSK500C2","-",500,1600,0.8,1200,"2-PSK",null,"1200HG1B",263,27]
["PSK500C4","-",500,3200,0.8,2600,"4-PSK",null,"2600HG1B",263,28]
["PSK500R","-",500,440,0.8,500,"1-PSKR",null,"500-HG1B",187,"-"]
["PSK500RC2","-",500,880,0.8,1400,"2-PSKR",null,"1400HG1B",263,24]
["PSK500RC3","-",500,1320,0.8,1900,"3-PSKR",null,"1900HG1B",263,25]
["PSK500RC4","-",500,1760,0.8,2600,"4-PSKR",null,"2600HG1B",263,26]
["PSK800C2","-",800,2300,0.8,1400,"2-PSK",null,"2300HGB1",263,57]
["PSK800RC2","-",800,1280,0.8,1400,"2-PSKR",null,"800HGB1C",263,54]
["PSK1000","-",1000,1600,0.8,1800,"1-PSK",null,"1800HG1B",263,50]
["PSK1000C2","-",1000,3200,0.8,3600,"2-PSK",null,"3600HG1B",263,52]
["PSK1000R","-",1000,880,0.8,1800,"1-PSKR",null,"1800HG1B",263,51]
["PSK1000RC2","-",1000,1760,0.8,3600,"2-PSKR",null,"3600HG1B",263,53]
["QPSK31","-","31,25",50,0.8,31,"1-QPSK",null,"31H0G1B",110,"-"]
["QPSK63","-","62,5",100,0.8,63,"1-QPSK",null,"63HG1B",3,"-"]
["QPSK125","-",125,200,0.8,125,"1-PQSK",null,"125HG1B",5,"-"]
["QPSK250","-",250,400,0.8,250,"1-PQSK",null,"250HG1B",127,"-"]
["QPSK500","-",500,800,0.8,500,"1-PQSK",null,"500HG1B","-","-"]
["RTTY 45","-",45,60,1,270,"2-FSK",null,"270HF1B",39,"-"]
["RTTY 50","-",50,66,1,270,"2-FSK",null,"270HF1B",40,"-"]
["RTTY 75","-",75,100,1,370,"2-FSK",null,"370HF1B",41,"-"]
["THOR4","+","3,9",14,1,173,"IFSK-18",null,"173HF1B",136,"-"]
["THOR5","+","5,4",22,1,244,"IFSK-18",null,"244HF1B",139,"-"]
["THOR8","+","7,8",28,1,346,"IFSK-18",null,"346HF1B",137,"-"]
["THOR11","+","10,8",40,1,262,"IFSK-18",null,"262HF1B",143,"-"]
["THOR16","+","15,6",58,1,355,"IFSK-18",null,"355HF1B",138,"-"]
["THOR22","+","21,5",78,1,524,"IFSK-18",null,"524HF1B",145,"-"]
["THOR25X4","+","24,3",88,1,1800,"IFSK-18",null,"1800HF1B",263,40]
["THOR50X1","+","48,6",176,1,900,"IFSK-18",null,"900HF1B",263,41]
["THOR50X2","+","48,5",176,1,1800,"IFSK-18",null,"1800HF1B",263,42]
["THOR100","+",97,352,1,1800,"IFSK-18",null,"1800HF1B",263,43]
["THROB1","-",1,10,0.8,72,"MFSK/AM",null,"72H0F1B",43,"-"]
["THROB2","-",2,20,0.8,72,"MFSK/AM",null,"72H0F1B",44,"-"]
["THROB4","-",4,30,0.8,144,"MFSK/AM",null,"144HF1B",45,"-"]
["THROBX1","-",1,10,0.8,94,"MFSK/AM",null,"94H0F1B",46,"-"]
["THROBX2","-",2,20,0.8,94,"MFSK/AM",null,"94H0F1B",47,"-"]
["THROBX4","-",4,40,0.8,188,"MFSK/AM",null,"188HF1B",146,"-"]

{"sheet":"Tabelle2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Tabelle3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}